**Dave Lennox Signature® Collection**

SLP98V Gas Furnace

*High Performance SLP98V Gas Furnace*

The multifunctional SLP98DF090XV60C furnace is easy to install and long lasting!

Downflow

**Energy Efficiency**

* Efficiency rating of up to 98.7% AFUE —can save your customers over $800 dollars each year\*, compared to standard furnaces
* ENERGY STAR® qualified—meets or exceeds EPA guidelines for energy efficiency
* This product has been designated as one of the Most Efficient ENERGY STAR qualified products in 2019. Products that are recognized as the Most Efficient of ENERGY STAR in 2019 prevent greenhouse gas emissions by meeting rigorous energy efficiency performance levels set by the U.S. Environmental Protection Agency
* Self-calibrating variable speed inducer—automatically adjusts to match the system requirements, ensuring cleaner combustion and efficient operation
* Stainless Steel secondary heat exchanger—has a robust, time-tested design that captures waste heat, allowing the furnace to achieve industry-leading efficiency levels
* Dual-fuel capability—can be combined with an electric heat pump to enhance comfort and fuel efficiency by alternating between electric and gas heat, optimizing energy use and minimizing heating costs
* iComfort™-enabled technology—allows the furnace, when installed with the easy-to-use programmable iComfort Wi-Fi® thermostat, to exchange information and make adjustments as needed to optimize performance and efficiency\*\*

**Quiet Operation**

* The quietest high-efficiency furnace!
* SilentComfort™ technology combines advanced engineering with sound-absorbing materials to deliver the ultimate in quiet performance
* Variable speed blower motor—provides a quiet, consistent flow of air for enhanced comfort, efficiency and humidity control
* Fully insulated cabinet—patented noise-reducing construction further minimizes operating sound to an industry-leading low level

**Home Comfort**

* Precise Comfort™ technology—automatically adjusts fan speed, heat and airflow capacity in increments as small as 1% for the ultimate in temperature control
* AirFlex™ technology—offers custom settings which can be selected to meet each home's specific year-round comfort requirements
* Zoning-compatible design—works with Lennox iHarmony™ zoning system to deliver the right amount of comfort for up to four zones
* Variable-capacity operation—goes beyond typical low and high two-stage operation, varying output from 35% to 100%

**Reliable Performance**

* High Quality Steel
* SureLight® igniter—silicone nitride construction ensures long product life and reliable operation
* SureLight control board (iComfort™ compatiable)—controls all furnace operations to ensure high reliability and efficiency. Direct-readout diagnostics for simple, quick troubleshooting